**Scenario 1: Understanding the Configuration and Working of HUB**

**A picture containing object

Description automatically generated**

**Assignment of IP Address:**

* **PC1:**
  + Click on PC1 select IP Configuration, assign IP address as **10.11.13.2** and subnet mask as **255.0.0.0** as shown below

**![A screenshot of a cell phone

Description automatically generated]()**

* + Repeat the for PC2, PC3, PC4 with IP’s: **10.11.13.3, 10.11.13.4, 10.11.13.5** andsubnet mask as **255.0.0.0**
  + Now press on Simulation Tab, send packet from PC1, to PC3.
  + Observe the movement of packet in the network topology using paly controls.